Darrin Chao

ITP 357

Homework 2

1. The largest packet is 1500 bytes. With larger packets, they are dropped.
2. The arp command on the Cisco router can display connections by each interface with more distributable MAC addressing.
3. Things work